**Hi,**

**Thanks so much for ordering a Tiny USB MIDI Knob! I hope you get as much use out of it as I do.**

**Instructions**

1. Plug it in using the supplied Micro-USB cable.
2. Your computer should recognize it as a device called ‘Tiny USB Knob’.
3. Click and Twist the knob to send Continuous Control MIDI notifications.

**Pro tip**

If you want to change the CC values that are sent when the knob is turned or clicked, go to [**https://midi.skilbeck.com**](https://midi.skilbeck.com). It should pick up the device automatically,

But if it doesn’t try clicking ‘Scan’ while your Tiny USB MIDI Knob is plugged in.

**Advanced users**

If you want to flash new firmware, click and hold the knob while you plug in the device. Once in flashing mode, you’ll have to either flash it with new firmware or unplug and plug it back in to get it back to normal mode.

**And…**

Small favour to ask – if you can bear it, would you mind awfully posting a Tweet about it? I don’t have a marketing budget (I don’t have any kind of budget at all, in fact), so getting the word out is kind of a challenge. Every mention helps! This QR code will get you started. Send me a link to any Social Media post for a 10% discount!



