**Hi,**

**Thanks so much for helping me test the Tiny USB Midi Knob!**

**Instructions**

1. Plug it in using a Micro-USB Type B cable.
2. Your computer should recognize it as a device called ‘Tiny Midi Knob’.
3. Twist or click the knob to send CC messages.
4. Configure the CC messages at <https://midi.skilbeck.com>

**NOTE**

**Please read this:** If your Tiny USB Midi Knob doesn’t work but flashes slowly after you’ve plugged it in, that means the USB connection failed. This is because your USB cable is a ‘Charger Only’ cable without data lines. Please use a data-enabled cable! If you suspect the cable, try another device with it to test it. If that also doesn’t work, it’s time to find another cable.

Please let me know how you get on?

You can email me: [midi@charlie.skilbeck.com](mailto:midi@charlie.skilbeck.com)

Or message me on Reddit (u/cskilbeck)

Or Tweet me @cskilbeck

Thanks again for your help – looking forward to hearing from you.

Charlie.